**ELEVATED SURFACES**

🞏 Are signs posted, when appropriate, showing the elevated surface load capacity?

🞏 Are surfaces that are elevated more than 48 inches provided with standard guardrails?

🞏 Are all elevated surfaces beneath which people or machinery could be exposed to falling objects provided with standard 4-inch toeboards?

🞏 Is a permanent means of access and egress provided to elevated storage and work surfaces?

🞏 Is required headroom provided where necessary?

🞏 Is material on elevated surfaces piled, stacked, or racked in a manner to prevent it from tipping, falling, collapsing, rolling, or spreading?

🞏 Are dock boards or bridge plates used when transferring materials between docks and trucks or railcars?