**FLOOR AND WALL OPENINGS**

🞏 Are floor openings guarded by a cover, a guardrail, or equivalent on all sides (except at stairways or ladder entrances)?

🞏 Are toeboards installed around the edges of permanent floor openings where persons may pass below the opening?

🞏 Are skylight screens able to withstand a load of at least 200 pounds?

🞏 Is the glass in windows, doors, glass walls, etc., subject to possible human impact, of sufficient thickness and type for the condition of use?

🞏 Are grates or similar type covers over floor openings such as floor drains designed to allow unimpeded foot traffic or rolling equipment?

🞏 Are unused portions of service pits and pits not in use either covered or protected by guardrails or equivalent?

🞏 Are manhole covers, trench covers and similar covers, and their supports designed to carry a truck rear axle load of at least 20,000 pounds when located in roadways and subject to vehicle traffic?

🞏 Are floor or wall openings in fire-resistant construction provided with doors or covers compatible with the fire rating of the structure and provided with a self-closing feature when appropriate?