**WALKWAYS**

🞏 Are aisles and passageways kept clear and marked as appropriate?

🞏 Are wet surfaces covered with non-slip materials?

🞏 Are holes in the floor, sidewalk, or other walking surface repaired properly, covered, or otherwise made safe?

🞏 Is there safe clearance for walking in aisles where motorized or mechanical handling equipment is operating?

🞏 Are materials or equipment stored in such a way that sharp projections will not interfere with the walkway?

🞏 Are spilled materials cleaned up immediately?

🞏 Are changes of direction or elevations readily identifiable?

🞏 Are aisles or walkways that pass near moving or operating machinery, welding operations, or similar operations arranged so employees will not be subjected to potential hazards?

🞏 Is adequate headroom provided for the entire length of any aisle or walkway?

🞏 Are standard guardrails provided wherever aisle or walkway surfaces are elevated more than 48 inches above any adjacent floor or the ground?

🞏 Are bridges provided over conveyors and similar hazards?