**FIRE PROTECTION**

🞏 Is your local fire department familiar with your facility, its location and specific hazards?

🞏 If you have a fire alarm system, is it certified as required and tested annually?

🞏 If you have interior standpipes and valves, are they inspected regularly?

🞏 If you have outside private fire hydrants, are they flushed at least once a year and on a routine preventive maintenance schedule?

🞏 Are fire doors and shutters in good operating condition?

🞏 Are fire doors and shutters unobstructed and protected against obstructions, including their counterweights?

🞏 Are fire door and shutter fusible links in place?

🞏 Are automatic sprinkler system water control valves, air and water pressure checked periodically as required?

🞏 Is the maintenance of automatic sprinkler systems assigned to responsible persons or to a sprinkler contractor?

🞏 Are sprinkler heads protected by metal guards if exposed to potential physical damage?

🞏 Is proper clearance maintained below sprinkler heads?

🞏 Are portable fire extinguishers provided in adequate number and type and mounted in readily accessible locations?

🞏 Are fire extinguishers recharged regularly with this noted on the inspection tag?

🞏 Are employees periodically instructed in the use of fire extinguishers and fire protection procedures?