**POWDER-ACTUATED TOOLS**

🞏 Are employees who operate powder-actuated tools trained in their use and required to carry a valid operator’s card?

🞏 Is each powder-actuated tool stored in its own locked container when not being used?

🞏 Is a sign at least 7 inches by 10 inches with bold face type reading “POWDER-ACTUATED TOOL IN USE” conspicuously posted when the tool is being used?

🞏 Are powder-actuated tools left unloaded until they are ready to be used?

🞏 Are powder-actuated tools inspected for obstructions or defects each day before use?

🞏 Do powder-actuated tool operators have and use appropriate PPE such as hard hats, safety goggles, safety shoes and ear protectors?